Connection Settings

Introduction:

Setting up the correct connection settings is crucial for establishing an internet connection. This support article provides a guide on the connection settings for NBN Connections for Superloop Fixed Wireless Connections.

NBN Connections:

Dynamic IP (Internet Protocol over Ethernet) is the common connection type used for NBN (National Broadband Network) Connections.

Superloop Fixed Wireless Connections:

PPPoE (Point-to-Point Protocol over Ethernet) is the standard connection type used for Fixed Wireless Connections.